{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["1 mg","0,1 mg","1 ppm"],"not_rendered":{"images":3,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1 mg","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"Which initial sample weight is needed for an IR moisture analyzer with 1 mg weight resolution?"]
[]
[]
[null,"Please key in the expected\nmoisture content of your sample:",{"v":1,"d":"1.00"},"%"]
[]
[null,"The minimum initial sample weight is:\n",{"v":10,"d":"10.00"},"g"]
[]
[null,"Accuracy of the analysis, using an initial\nsample weight below 5 g:",{"v":0.8,"d":"0.80"},"to",{"v":1.2,"d":"1.20"},"%"]
[null,"Accuracy of the analysis, using an initial\nsample weight below 5 g:",0.95,"to",1.05,"%"]

{"sheet":"0,1 mg","index":1,"n_rows":14,"n_cols":6,"rows_kept":14,"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"Which initial sample weight is needed for an IR moisture analyzer with 0.1 mg weight resolution?"]
[]
[]
[null,"Please key in the expected\nmoisture content of your sample:",{"v":1,"d":"1.00"},"%"]
[{"$nulls":3},"mg"]
[null,"The minimum initial sample weight is:\n(a minimum of 90 mg is required for all cases)",{"v":1,"d":"1.00"},"g"]
[]
[null,"Accuracy of the analysis, using an initial\nsample weight below 5 g:",0.95,"to",1.05,"%"]
[null,"Accuracy of the analysis, using an initial\nsample weight below 5 g:",0.98,"to",1.02,"%"]

{"sheet":"1 ppm","index":2,"n_rows":14,"n_cols":6,"rows_kept":14,"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"Which initial sample weight is needed for a coulometer with 1 ppm resolution?"]
[]
[]
[null,"Please key in the expected\nmoisture content of your sample:",{"v":1.17,"d":"1.1700"},"%  = ",11700,"ppm"]
[]
[null,"The minimum initial sample weight is:\n(an initial sample weight less than 5 mg is not useful)",{"v":25.641025641025646,"d":"25.64"},"mg"]
[]
[null,"Accuracy of the analysis:",{"v":1.1465999999999998,"d":"1.1466"},"to",1.1934,"%"]
[null,null,{"v":11465.999999999998,"d":"11466"},"to",11934,"ppm"]